{"text_format":"3","workbook":"xls","n_sheets":1,"sheets":["通力报价"],"not_rendered":{"external_links":1,"defined_names":1},"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"通力报价","index":0,"n_rows":9,"n_cols":8,"rows_kept":9,"merged":[[0,0,0,7],[2,10,8,10],[8,0,8,5]],"flags":["formulas_cached_only"]}
["人才院电梯拆除及采购安装项目采购清单",null,null,"","","","",""]
["序号","名称","参数及规格","单位","数量","单价（元）","合价（元）","备注\n（品牌）"]
[1,"原电梯拆除","载重1000kg，层站5层5站（其中一台不下地下室），原电梯拆除后负责运输到业主定位位置，残值归业主所有","台",2,null,{"v":0,"d":"0.00"}]
[2,"井道整改","吊钩，圈梁，门头梁，地坎整改","项",1,null,{"v":0,"d":"0.00"}]
[3,"洞口及地坎修补","如地坎石，装饰门套产生破损，中标单位负责修补。控制柜孔及外呼孔的修补","项",1,null,{"v":0,"d":"0.00"}]
[4,"新电梯采购","载重1000kg，\n速度1.6m/s，\n5层5站（其中一台不下地下室）\n开门尺寸900*2200，\n轿厢净高2400\n厅门，轿门，轿壁，吊顶发纹不锈钢，大理石地板\n无障碍及消防按照规范配置\n","台",2,null,{"v":0,"d":"0.00"}]
[5,"新电梯安装，调试，验收","载重1000kg，层站5层5站（其中一台不下地下室）","台",2,null,{"v":0,"d":"0.00"}]
[6,"新电梯轿厢精装","发纹不锈钢吊顶（灯带+亚克力透光板）\n岩石灰大理石地板\n轿厢2侧壁及后壁中板自然橡木饰钢板，后壁两侧板镜面不锈钢","台",2,null,{"v":0,"d":"0.00"}]
["总价（元）",{"$nulls":5},{"v":0,"d":"0.00"}]